|  |  |
| --- | --- |
| Power-up, 1st time  Before connected  (Factory settings) | Controls disabled  Dip override disabled  All user eq’s are flat: Peak, 1kHz,0.00dB,Q1.4  Active Preset, HF/LF trim determined by dip switch.  Trim level is 0dB, encoder adjusts trim level  DIM disabled  LED, Standby, Amp Fault, Limiter Engaged Enabled |
| Power-up, 2nd time and after  Before connected  (Stored settings) | Controls disabled  Dip override is last set  . disabled - user/preset eq’s by dip switch  . enabled - last selected  Trim level, DIM are last set. They could be set by encoder or controller |
| Controller connected |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |